NOTE: CN19 shown with out-of-order VR7, VR8 and VR6 used to bias V6, V7 and V8, resp.

