Main B+ high-voltage measuring point, minus is Chassis Gnd.



Chassis Gnd

Main AC fuse F1

Main DC B+ 500Vdc

Main B+ can be measured at or across C30 as shown or, at or across C3 at opposite side of board.