CN18 male pin out



Bias Common “TP-Gnd” for V3, 4 and 5. Use bias harness female end for meter leads as per the SE-40 manual.

Note the TPs get reversed in the cable harness and are correct as shown in the manual.

TP1