SE-40 View when upside-down, sitting on its transformers with all tubes removed and labeled (per corrected tube map) and bottom plate removed.



Remove all circuit board mounting screws around the board’s periphery and in-board screws, if any – typically 10 screws.

Very important B+ power supply minus to Chassis metal “Star” GND mounting screw.