Metalized polypropylene MKP “Fast Cap” installed across B+ Main.



Install new non-polarized

Solen 12uF 630V “C3”

C51 (Yellow)

Remove and discard