Once the circuit board is free to move, remove the connections to the front panel power switch and carefully back-out the green LED from its hole.



These two power switch connectors should be small, push-on tab types so gently pull rearward and wiggle them off.