D9



OEM R55 = 1ohm, 5Watt

Replacement = 2ohm, 5W (any type)

OEM D9 = 6Amp rectifier bridge, 200V or better.

Replacement = 8Amp version, same body-style and footprint