

Front panel power switch push-on connectors

R29 and R10 (Grn Brwn Org Gld)

Replace each with 51.0kΩ 1% 2W