

Optional:

100pF silver-mica C20 and C13 bypass caps across C14 and C19, 0.22uF V1=>V2 R & L channel couplers.

Remove and keep or lift one leg. These can add some unwelcome brightness and are removed in Jeff’s and Loc’s mods.