D9 and R55 – associated with V1 and V2’s 6.3Vdc heater supply.



OEM R55 = 1Ω, 5Watt

Replacement = 2Ω, 5W (any type)

OEM D9 = 6Amp rectifier bridge, 200V or better.

Replacement = 8Amp version, same body-style and footprint

BUY: D9 at Mouser, qty 1 per amp

<http://www.mouser.com/ProductDetail/Rectron/RS803/?qs=sGAEpiMZZMtQ8nqTKtFS%2fNgL6ac11fJu2VJeg40E%2fC0%3d>